LEHIGH ACRES SIGN STANDARDS FOR LED SIGNS
In an effort to give commercial and industrial uses, within the Lehigh Acres Planning Community, the ability to broadcast their business or message to the general public, LED lit signs shall be permitted throughout the commercial/industrial community.
Strict adherence to sign standards for light emitting signs shall keep visual sign clutter to a minimum and cause the driving public to have a minimum of distraction.
Variance from the standards set forth herein, shall not be permitted, except under the most unusual of circumstances.
· LOCATION
1. LED lighted signs shall be permitted on commercially / industrially zoned business properties containing three or more parcels.
2. LED lighted signs shall be permitted on commercially / industrially zoned corner properties of two or more parcels.
3. LED lighted signs shall be permitted to be erected at lot corners, mid-property or at property entrances.
4. Where properties have more than one entrance, either on the same street, or two streets, only one LED sign shall be permitted.
· SIZE
1. Signs lit by LED lights shall be a maximum of four (4) feet high by eight (8) feet wide. 
2. Signs may be two-faced, a maximum of four (4) feet high by eight (8) feet wide on each face.
3. Signs mounted to display price per gallon at fuel pumps, shall be mounted on the flat side of the fascia, but in no case exceed four (4) feet in height.


· MOUNTING
1. Signs lit by LED lights shall be mounted in a monument sign, the top of which shall be no higher than six (6) feet above the adjacent grade. Single pole or pylon signs shall be prohibited.
2. Monument signs containing LED lights shall be architecturally compatible with the building structure(s).
3. Monument signs shall only contain the LED message board. No other message shall be mounted on the monument sign.
4. All monument signs containing LED lights shall have the street address mounted prominently at the top of the sign, in a contrasting color to the sign, and visible from each direction of travel.
· MESSAGES
1. For single occupancy businesses, the name of the business, the logo for the business, and the product the business sells, may be displayed.
2. For single occupancy businesses, the message displayed by the LED lights shall not flash, change colors, change messages, or shall not create any other distractions for motorists.
3. For multi-tenant businesses, the LED message center may alternate business names within the prescribed area of the LED lighting.
4. When utilizing an alternating business name sign in LED lighting, there shall be no other display of business names or messages anywhere else on the monument sign.
5. There shall be no sound emitted from LED signs.
6. There shall be no other banners, flags, pennants or signs mounted from the LED monument sign or from other locations on the property.
· LANDSCAPING
1. All monument signs containing LED lighting shall have landscaping provided in the open area below the LED face. 
2. Landscaping shall consist of shrubs, perennials or other materials that shall enhance the general appearance of the sign.
3. Landscaping shall be maintained for the duration of the life of the sign.
4. There shall be one tree provided on one side of the monument sign to further enhance the general appearance of the sign. Trees may be multi-branched palms, deciduous, flowering or groupings of palms.
5. Trees shall be maintained for the duration of the life of the sign.
· INTENSITY
1. The intensity of the light being emitted from the LED signboards shall be measured in……..
· CODES
1. All LED signs and the accompanying monument structure shall comply with all current building and electrical codes.
2. All LED signs and accompanying monument structure shall receive a building permit from the appropriate permitting agency.
· MODIFICATIONS
1. These LED sign standards may be modified from time to time upon notification of the public and through a public hearing process.
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